**Protection layer order requirement**

Requirement:

1. Thickness 0.2mm +/-0.04mm
2. FR4 boards with copper on one side
3. Copper thickness 17 μm
4. Halogen free
5. Size tolerance +/-0.2mm
6. Holes position tolerance +/-0.2mm
7. Holes diameter -0.0mm +0.1mm

Order quantity and types

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| type | machined | Raw material | destination | Package size |
| QS1 | 40 | 40 | Chile | 1370\*780\*160 |
| QS3 | 80 |  | 50%Canada 50% Israel | 1430\*1050\*180 |
| QL1 | 80 | 10 | Israel | 1390\*1230\*200 |
| QL2 | 80 |  | Canada | 1830\*1320\*200 |

Destination address for transportation:

Israel:

Meir Shoa
Physics department
Weizmann Institute of Science

234 Herzl Street,

 Rehovot 7610001

Israel
Tel. +972542638904

Canada

Glen Ford
Physics Department, Carleton University
1125 Colonel By Drive
Ottawa, Ontario, K1S 5B6
Canada
Tel: (613)295-0198

Chile:

Ms. Nicole Milla
UNIVERSIDAD TECNICA FEDERICO SANTA
MARIA
Avda Espana 1680
CL - 110-V VALPARAISO
CHILE
Tel：+56 32 2654939 +56 32 2654827

Add material description code in the invoice: CCTVal FB0821 RUT:81.668.700-4